# RP Registration Discard Statistics

1. Right click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Statistics button.

4. Select category CDMA PDSN PCF & SO Based Statistics.

5. Select a row and click on RP Registration Statistics Button and from the Category select RP Registration Discard Statistics.

The following information appears:

> Initial A11 Registration Requests Discarded (cCdmaPcfSoRpInitRegDiscardedReqs)

> A11 Re-registration Request Discarded (cCdmaPcfSoRpReRegDiscardedReqs)

> A11 De-registration Request Discarded (cCdmaPcfSoRpDeRegDiscardedReqs)

> Handoff A11 Registration Requests Discarded (cCdmaPcfSoRpHandoffRegDiscardedReqs)

### Initial A11 Registration Requests Discarded (cCdmaPcfSoRpInitRegDiscardedReqs)

Number of Initial A11 Registration requests silently discarded since the system was last restarted.

### A11 Re-registration Request Discarded (cCdmaPcfSoRpReRegDiscardedReqs)

Number of A11 Re-Registration requests silently discarded since the system was last restarted.

### A11 De-registration Request Discarded (cCdmaPcfSoRpDeRegDiscardedReqs)

Number of A11 De-Registration requests silently discarded since the system was last restarted.

### Handoff A11 Registration Requests Discarded (cCdmaPcfSoRpHandoffRegDiscardedReqs)

Number of handoff A11 Registration requests silently discarded since the system was last restarted.