# Serial Statistics

The CiscoView Monitor Port dialog box displays the following information:

Checksum Err Pkts (locIfInCRC)

Aborted Pkts (locIfInAbort)

Misaligned Pkts (locIfInFrame)

Carrier Sig Trans (locIfCarTrans)

Overruns (locIfInOverrun)

Aborted Pkts (locIfInAbort)

Number of input packets that were aborted.

Carrier Sig Trans (locIfCarTrans)

Number of times the interface detected the carrier signal transition.

Overruns (locIfInOverrun)

Shows the amount of input that arrived too quickly for the hardware to receive.

Checksum Err Pkts (locIfInCRC)

Number of input packets that had cyclic redundancy check (CRC) errors.