# IP Precendence-to-DSCP Mapping

Configuration > Mapping Tables > IP Prec >DSCP

Configure DSCP values for each IP Precedence. This table is applicable if trust state is trustIpPrec.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- IP Prec (caqIpPrecToDscpIpPrec)

- DSCP Value (caqIpPrecToDscpDscp)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access the online help.

IP Prec (caqIpPrecToDscpIpPrec)

The IP Precedence value being mapped to the DSCP value in this device.

DSCP Value (caqIpPrecToDscpDscp)

The DSCP value to which the IP Precedence value maps.