# Weighted Round Robin (WRR)

Configuration > Output Scheduling > WRR

Weighted Round Robin (WRR) uses weight value to decide how much to transmit from one queue before switching to another. The higher the weight assigned to a queue, the more transmit bandwidth allocated to it.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Direction (caqQueueDirection)

- Queue Type (caqQueueType)

- Queue Number (caqQueueNumber)

- WRR Weight (caqQueueWrrWeight)

- Buffer Size Ratio (%) (caqQueueBufferSizeRatio)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access the online help.

Direction (caqQueueDirection)

Indicates whether this row's queue parameters are to be applied for ingress (incoming) or egress (outgoing) traffic.

Queue Type (caqQueueType)

Indicates queue type.

Queue Number (caqQueueNumber)

Indicates queue number.

WRR Weight (caqQueueWrrWeight)

Allows you to configure the weight for the specified queue type and direction.

Buffer Size Ratio (%) (caqQueueBufferSizeRatio)

Indicates the percentage of ingress or egress packet buffer memory allocated to the specified queue.