# SRP Ring Topology Table

Use this option to view specific information about a particular node on SRP ring.

## Procedure

To access SRP ring topology information:

1. Double-click or right-click the port and select Configure from the pop-up menu.

2. Select SRP Ring Topology Table from the Category menu to display SRP ring topology configuration information.

SRP Ring Topology Table dialog box displays:

> Hops from LocalNode (srpNodeHopsNumber)

> MAC Address (srpNodeMACAddress)

> Wrapped State (srpNodeWrapped)

> Node Name (srpNodeName)

## Related Topics

Using CiscoView Interface

Using the Main Menu

Selecting Components

Configuring Devices and Components

Monitoring Devices and Components

### Hops from LocalNode (srpNodeHopsNumber)

Number of hops from local node to another node counted clockwise.

Value is between 0 and (srpNodesOnTheRing - 1).

### MAC Address (srpNodeMACAddress)

MAC Address of SRP node.

### Wrapped State (srpNodeWrapped)

Shows whether node is wrapped.

### Node Name (srpNodeName)

Displays node name reported by SRP.

Blank if node name is unknown.