# LAPB Status

The following LAPB status information is displayed:

Oper Station Type

Oper Port ID

LAPB Protocol Ver.

LAPB State Changes

LAPB State Chg Reason

# Oper Station Type (lapbAdmnStationType)

Displays the station type. Possible values are DTE, DCE, or DXE.

# Oper Port ID (lapbOperPortId)

Displays the port number of the supporting physical interface.

# LAPB Protocol Ver (lapbProtocolVersion)

Displays an object identifier that identifies the LAPB protocol version being used. For example, the value 1.3.6.1.2.10.10.16.5.3 indicates that the version being used is the 1984 CCITT version.

# LAPB State Changes (lapbFlowStateChanges)

This counter displays the number of LAPB state changes, including resets.

# LAPB State Chg Reason (lapbFlowChangeReason)

Specifies the reason for the most recent LAPB state change.