# GGSN GTP

The GGSN GTP category of the Chassis Monitoring dialog box lists GGSN GTP statistics.

Note This dialog can be viewed if cGtpGSNService is set to 'ggsn'.

## Procedure

1. Right-click the device and then select Monitor.

2. Select GGSN GTP from the Category list.

The following information appears:

No of Failures (cGtpPathFailureOccurrences)

GTP Packets Dropped (cGtpTotalDroppedPackets)

### No of Failures (cGtpPathFailureOccurrences)

Number of times that any one of the GSN's peers failed to respond to a GTP Echo Request message during the waiting intervals.

### GTP Packets Dropped (cGtpTotalDroppedPackets)

Total number of GTP packets that were received but could not be processed and hence were dropped since system started.