# Mobile Node Registration Flags Configs

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. Select category Mobile Node Registration Flags Configs.

The following information appears:

> Agent IP Address (mnRegAgentAddress)

> COA (mnRegCOA)

> Mobile Node Registration Flags (cmiMnRegFlags)

### Agent IP Address (mnRegAddress)

Mobile node address.

### COA (mnRegCOA)

Mobile node care-of-address.

### Mobile Node Registration Flags (cmiMnRegFlags)

Registration flags sent by the mobile node. It is the second byte in the Mobile IP Registration Request message.