# Home Agent Registration Processing Statistics-Registration Requests

1. ## Right-click on the MWAM Card and select Configure.

2. ## Select category MWAM module.

3. ## Select a row and click the Statistics button.

4. ## Select category Home Agent Registration Processing – Registration Requests.

The following information appears:

> Registration Requests (cmiHaRegTotalProcLocRegs)

> Max Requests (cmiHaRegMaxProcLocInMinRegs)

> Requests Processed (cmiHaRegProcLocInLastMinRegs)

> Processed by HA (cmiHaRegTotalProcByAAARegs)

> Maxi Processing by HA per Min (cmiHaRegMaxProcByAAAInMinRegs)

> Last Minute Processing by HA (cmiHaRegProcAAAInLastByMinRegs)

> Requests Received by HA (cmiHaRegRequestsReceived)

> Requests Denied by HA (cmiHaRegRequestsDenied)

> Requests Discarded by HA (cmiHaRegRequestsDiscarded)

### Registration Requests (cmiHaRegTotalProcLocRegs)

Total number of registration requests processed by the home agent. Includes only those registration requests that were authenticated locally by the home agent.

### Max Requests (cmiHaRegMaxProcLocInMinRegs)

Maximum number of registration requests processed in a minute by the home agent. It includes only those registration requests that were authenticated locally by the home agent.

### Requests Processed (cmiHaRegProcLocInLastMinRegs)

Number of registration requests processed during the last minute by the home agent. It includes only those registration requests that were authenticated locally by the home agent.

### Processed by HA (cmiHaRegTotalProcByAAARegs)

Total number of registration requests processed by the home agent. Includes only those registration requests that were authenticated by the AAA server.

### Maximum Processing by HA (cmiHaRegMaxProcByAAAInMinRegs)

Maximum number of registration requests processed in a minute by the home agent. Includes only those registration requests that were authenticated by the AAA server.

### Last Minute Processing by HA (cmiHaRegProcAAAInLastByMinRegs)

Number of registration requests processed by the home agent in the last minute. Includes only those registration requests that were authenticated by the AAA server.

### Requests Received by HA (cmiHaRegRequestsReceived)

Total number of registration requests received by the home agent. Includes initial registration requests, re-registration requests and de-registration requests.

### Requests Denied by HA (cmiHaRegRequestsDenied)

Total number of registration requests denied by the home agent. Reasons for which a home agent denies a request include:

1. Can't allocate IP address for mobile node.
2. Request parsing failed.
3. NAI length exceeds the packet length.

### Requests Discarded by HA (cmiHaRegRequestsDiscarded)

Total number of registration requests discarded by the home agent. The reasons for which HA discards a request include:Total number of Registration Requests discarded by the home agent.

Reasons for which a home agent discards a request include:

1. IP mobile home-agent service is not enabled.
2. HA-CHAP authentication failed.
3. Mobile node security association retrieval failed.