# SSG Service Route Table

The SSG Service Route Table category of the Configure dialog box displays details on the service selection gateway (SSG) service route table.

## Procedure

1. Right-click the device, then select Configure, or double-click the device.

2. Select SSG Service Route Table from the Category list.

The following information appears:

Service Name (cssgServiceName)

Service Route Type (cssgServiceRouteType)

Service Route Address (cssgServiceRouteAddr)

Service Mask Type (cssgServiceRouteMaskType)

Service Mask Address (cssgServiceRouteMask)

Service Action (cssgServiceRoutePermission)

### Service Name (cssgServiceName)

Name of the service profile.

### Service Route Type (cssgServiceRouteType)

Value that represents the type of address stored in cssgServiceServRouteAddr.

### Service Route Address (cssgServiceRouteAddr)

IP address of the networks available to you.

### Service Mask Type (cssgServiceRouteMaskType)

Value that represents the type of address stored in cssgServiceServRouteMask.

### Service Mask Address (cssgServiceRouteMask)

Mask to be combined with the destination address before the destination address is compared to the value in cssgServiceRouteAddr.

### Service Action (cssgServiceRoutePermission)

Action to be taken on packets when the destination address matches with the cssgServiceRouteAddr.

Action can be:

Value | Description
1 | permit
2 | deny