# Address Allocated Config

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. Select category Address Allocated Config.

The following information appears:

> Pool Name (cIpLocalPoolName)

> Local Pool Address Type (cIpLocalPoolAllocAddrType)

> Inet Address (cIpLocalPoolAllocAddr)

> Allocation Interface (cIpLocalPoolAllocIfIndex)

> Allocation Person (cIpLocalPoolAllocUser)

Pool Name (cIpLocalPoolName)

A non-empty string that uniquely identifies an IP local pool.

### Local Pool Address Type (cIpLocalPoolAllocAddrType)

Address type of cIpLocalPoolAllocAddr.

### Inet Address (cIpLocalPoolAllocAddr)

Allocated IP address. The address type of this object is described by cIpLocalPoolAllocAddrType.

### Allocation Interface (cIpLocalPoolAllocIfIndex)

Interface from which the allocation message was sent. If the interface cannot be determined, the value of this object will be zero.

### Allocation Person (cIpLocalPoolAllocUser)

User name of the person from whom the allocation message was sent.