# SSG Server & Port Group

This dialog box displays details on the Service Selection Gateway (SSG) server and port group.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select SSG Server & Port Group from the Category list.

The following information is displayed:

> Redirect-Group Name (cssgTcpRedirectGrpName)

> Port Group Name (cssgTcpRedirPortMapGrpName)

> Server Port Group RowStatus (cssgTcpRedirPortGrpMapRowStat)

### Redirect-Group Name (cssgTcpRedirectGrpName)

Name of the redirect-group.

### Port Group Name (cssgTcpRedirPortMapGrpName)

Name of the port group.

A port group is a set of ports that can be associated with a TCP redirect group for traffic redirection.

### Server Port Group RowStatus (cssgTcpRedirPortGrpMapRowStat)

Status of the table entry. Change the status to create a new table entry or delete an existing one.

- To create a row, set the object to createAndGo. There are no mandatory objects in a create request.

- To delete a row, set the object to destroy.