# SSG Port Server Association

This dialog box displays details on the Service Selection Gateway (SSG) port server association.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select SSG Port Server Association from the Category list.

The following information is displayed:

> Redirect-Group Name (cssgTcpRedirectGrpName)

> Server Group Port Number (cssgTcpRedirPortNo)

> Port Server Association RowStatus (cssgTcpRedirPortNoMapRowStat)

### Redirect-Group Name (cssgTcpRedirectGrpName)

Name of the redirect group.

### Server Group Port Number (cssgTcpRedirPortNo)

Port number associated with the server group.

### Port Server Association RowStatus (cssgTcpRedirPortNoMapRowStat)

Status of the table entry. Change the status to create a new table entry or delete an existing one.

- To create a row, set the object to createAndGo. cssgTcpRedirPortNo is a mandatory object for a create request.

- To delete a row, set the object to destroy.