# Monitoring SONET Path Current Statistics

Select SONET Path Current Statistics from the Monitor pull-down menu to monitor SONET path statistics collected for the current 15 minute interval. The following values are displayed:

Errored Seconds (sonetPathCurrentESs)

Severely Errored Seconds (sonetPathCurrentSESs)

Unavailable Seconds (sonetPathCurrentUASs)

Code Violation (sonetPathCurrentCVs)

### Errored Seconds (sonetPathCurrentESs)

The number of seconds during the current 15 minute interval that a path error occurred for this path.

### Severely Errored Seconds (sonetPathCurrentSESs)

The number of seconds during the current 15 minute interval that a severe path error occurred for this path.

### Code Violation (sonetPathCurrentCVs)

The number of seconds during the current 15 minute interval that a coding violation occurred for this path.

### Unavailable Seconds (sonetPathCurrentUASs)

The number of seconds during the current 15 minute interval that the path was not available.