# Switch Acceleration

Supervisor II Card>Configure>Switch Acceleration

Switch Acceleration (switchAccelerationModuleEnable)

Indicates whether switch acceleration is enabled on this module.

If the ifAdminStatus of any port on this module is set to "up", this feature cannot be enabled. When the ifAdminStatus of all ports on this module is set to "down", the system will increase the switching bandwidth when this feature in enabled.

Note: Enabling/disabling this feature may affect performance for 1-2 seconds.

Click OK to continue. Click Apply to save the changes in the dialog box. Click Cancel to close the dialog box. Click Refresh to update the contents of the dialog box. Click Print to print the contents of the dialog box. Click Help to access online help.