# COPS Device Configuration

Device>Configure>Cops

Max. # of Servers (ccopsServerMax)

Maximum number of configurable COPS servers allowed for each client type. A value of zero indicates no limitation on the number of configurable COPS servers.

Max. # of Roles (ccopsMaxRole)

The maximum number of role-combinations supported by this device. a value of zero indicates no limitation on the number of role-combinations. Each CopsRoleCombination may contain up to ccopsMaxRole roles.

Max. # of role Combinations (ccopsMaxRoleCombination)

The maximum number of role-combinations supported by this device. A value of zero indicates no limitation on the number of role-combinations. Each CopsRoleCombination may contain up to ccopsMaxRole roles.

Initial Time-out (ccopsInitialTimeout)

This value is used for the first retry after every successful connnection.

Time-out Increment of Next Retry (ccopsTimeoutIncrement)

On every consecutive failure to connect to all existing COPS server for a client type, the COPS client increases the retry time-out by ccopsTimeoutIncrement but not greater than ccopsTimeoutMax.

Max. Time-out (ccopsTimeoutMax)

The maximum retry time-out that the COPS client allows.