# Mobile Node Registration Flag Configs

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.

2. Select Mobile Node Registration Flag Configs from the Category list.

The following information appears:

> Agent IP Address (mnRegAgentAddress)

> COA (mnRegCOA)

> Mobile Node Registration Flags (cmiMnRegFlags)

### Agent IP Address (mnRegAgentAddress)

The IP address of the agent as used in the destination IP address of the Registration Request. The agent may be a home agent or a foreign agent.

### COA (mnRegCOA)

The Care-of address for the registration.

### Mobile Node Registration Flags (cmiMnRegFlags)

Registration flags sent by the mobile node. It is the second byte in the Mobile IP Registration Request message.