# Voice Port Interface Dialog

Port>Configure>Voice Configuration>Voice Port Interface

The first two MIB variables are represented in table format.

Operational DNS Server (voicePortOperDnsServerIpAddr)

Operational DNS server of this port.

Operational DNS Server Source (voicePortOperDnsServerSource)

Source of the DNS server IP address for this port.

Port IP Address (voicePortIfIpAddress)

IP address for this port.

Port IP Mask (voicePortIfIpNetMask)

Subnet mask for this port.

Port IP Gateway (voicePortIfGatewayAddress)

Router address for this port.

Port TFTP Server (voicePortIftftpServerAddress)

TFTP server address for this port.

Port DNS Server (voicePortIfdnsServerAddress)

DNS server address for this port.

Port DNS Domain (voicePortIfdnsDomain)

Domain name for this port.

Port Operational DNS Domain (voicePortIfOperDnsDomain)

Operational DNS domain name for this port.

DHCP Service (voicePortIfDHCPEnabled)

Indicates whether DHCP service is enabled.