# RP Registration Failures

From this dialog box, you can view Packet Control Function (PCF) and Service Option (SO)-based RP registration failures.

## Navigation

1. Right-click the Mobile Wireless Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN PCF & SO Based Statistics.

4. With an entry selected in the PCFs & Service Options table, click RP Registration Statistics.

5. Select RP Registration Failures.

The following information is displayed:

> Unknown Failures (cCdmaPcfSoRpRegPcfUnknwnFails)

> Administrative Failures (cCdmaPcfSoRpRegAdmnFails)

> Insufficient Resource Failures (cCdmaPcfSoRpRegNoRsrcFails)

> MN Authentication Failures (cCdmaPcfSoRpRegMNAuthFails)

> ID Mismatch Failures (cCdmaPcfSoRpRegIdMismatFails)

> Bad Request Failures (cCdmaPcfSoRpRegBadReqFails)

### Unknown Failures (cCdmaPcfSoRpRegPcfUnknwnFails)

Number of registration requests that failed when the PCF address did not appear in the Packet Data Serving Node's (PDSN) list of configured PCFs for an unspecified reason since system startup.

### Administrative Failures (cCdmaPcfSoRpRegAdmnFails)

Number of registration requests that failed when the PCF address did not appear in the PDSN's list of configured PCFs since system startup.

### Insufficient Resource Failures (cCdmaPcfSoRpRegNoRsrcFails)

Number of registration requests that failed when either the number of PCFs or sessions reached the maximum value or system resources were insufficient since system startup.

### MN Authentication Failures (cCdmaPcfSoRpRegMNAuthFails)

Number of registration requests that failed due to a Mobile Node (MN) authentication failure since system startup.

### ID Mismatch Failures (cCdmaPcfSoRpRegIdMismatFails)

Number of registration requests that failed due to an identification mismatch since system startup.

### Bad Request Failures (cCdmaPcfSoRpRegBadReqFails)

Number of registration requests that failed due to a badly formed request since system startup.