# Encryption Configuration

The following encryption configuration information can be displayed:

Configured algorithms

Encryption key timeout

Number of encryption engines

Number of connections

# Configured Algorithms

The type of configuration configured on this router. Supported algorithm types include:

56-bit DES with 64-bit cipher feedback

56-bit DES with 8-bit cipher feedback

40-bit DES with 64-bit cipher feedback

40-bit DES with 8-bit cipher feedback

A single router can support more than one algorithm type at the same time.

# Encryption Key Timeout

The interval (in minutes) after which keys expire for a session and must be renegotiated.

# Number of Encryption Engines

The total number of encryption engines on this router.

# Number of Connections

The total number of crypto connections, including active, pending, and dead connections.