# Home Agent Redundancy Statistics - Acknowledgement

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Statistics button.

4. Select category Home Agent Redundancy Statistics Contd1.

The following information appears:

> Ack Received (cmiHaRedunReceivedBIAcks)

> Ack Dropped (cmiHaRedunDroppedBIAcks)

> Security Violations (cmiHaRedunSecViolations)

### Ack Received (cmiHaRedunReceivedBIAcks)

Total number of acknowledgements received in response to binding information replies sent by the home agent.

### Ack Dropped (cmiHaRedunDroppedBIAcks)

Total number of acknowledgements dropped by the home agent since there are no corresponding binding information replies sent by it.

### Security Violations (cmiHaRedunSecViolations)

Total number of security violations in the home agent caused by processing of the packets received from the peer home agent. Security violations can occur for the following reasons.

- Authenticator value in the packet is invalid.
- Value stored in the identification field of the packet is invalid.