# SSG TCP Redirect Group

The SSG TCP Redirect Group category of the Configure dialog box displays details on the service selection gateway (SSG) TCP redirect group.

## Procedure

1. Right-click the device, then select Configure, or double-click the device.

2. Select SSG TCP Redirect Group from the Category list.

The following information appears:

Redirect-Group Name (cssgTcpRedirectGrpName)

Redirect Server Type (cssgTcpRedirectGrpServerAddrType)

Redirect Server (cssgTcpRedirectGrpServerAddr)

Redirection port (cssgTcpRedirectGrpServerPort)

Redirection Row Status (cssgTcpRedirectGrpRowStatus)

### Redirect-Group Name (cssgTcpRedirectGrpName)

Name of the redirect group.

### Redirect Server Type (cssgTcpRedirectGrpServerAddrType)

Value that represents the type of address stored in cssgTcpRedirectGrpServerAddr.

### Redirect Server (cssgTcpRedirectGrpServerAddr)

IP address of the server in the server group.

### Redirection port (cssgTcpRedirectGrpServerPort)

Port of the server to which TCP traffic is to be redirected.

### Redirection Row Status (cssgTcpRedirectGrpRowStatus)

The status of the table entry.

Status can be used to create or delete conceptual rows in the table.

To create a row, set the object to createAndGo. There are no mandatory objects in a create request.

To delete a row, set the object to destroy.