# GGSN GTP

From this dialog box, you can view GGSN GTP statistics.

Note: This dialog box is available only if the value of cGtpGSNService is set to ggsn.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Statistics.

4. Select GGSN GTP from the Category drop-down box.

The following information is displayed:

> No of Failures (cGtpPathFailureOccurrences)

> GTP Packets Dropped (cGtpTotalDroppedPackets)

### No of Failures (cGtpPathFailureOccurrences)

Number of times that any one of the GSN's peers failed to respond to a GTP Echo Request message during the waiting intervals.

### GTP Packets Dropped (cGtpTotalDroppedPackets)

Total number of GTP packets that were received but could not be processed and hence were dropped since system started.