# Server Farm Info

This dialog box provides details about the server farms, such as the name of the server farm, details of the algorithm configured on the server farm, bind identification number, and the number of real servers present in the server farm.

## Procedure

1. Right-click the device, then select Configure > SLB Statistics.

2. With a server load balancing (SLB) instance selected, click Server Farm. The following information is displayed:

> Farm Name (slbServerFarmName)

> Farm Predictor (slbServerFarmPredictor)

> Nat (slbServerFarmNat)

> No. of Real Servers (slbServerFarmNumberOfRealServers)

> Bind Identification (slbServerFarmBindId)

> Server Row Status (slbServerFarmRowStatus)

### Farm Name (slbServerFarmName)

The name of server farm.

### Farm Predictor (slbServerFarmPredictor)

The load balancing algorithm for the local SLB entity used by the server farm for its real servers.

### Nat (slbServerFarmNat)

The type of network address translation (NAT) used by the local SLB entity for servers in this server farm.

### No. of Real Servers (slbServerFarmNumberOfRealServers)

The number of real servers in this server farm.

### Bind Identification (slbServerFarmBindId)

Bind Identification is used to identify one or more real servers for which slbDfpRealWeight applies to the slbRealOperWeight of the real server.

Rows in slbServerFarmTable for which slbServerFarmBindId matches slbDfpRealBindId are identified.

### Server Row Status (slbServerFarmRowStatus)

The management station uses row status to create or delete the row entry in slbServerFarmTable following the RowStatus textual convention.