# Rejected PDP Statistics per Cause - 2

## Procedure

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category list.

3. Select a row and click Statistics.

4. Select Rejected PDP Statistics per Cause - 2 from the Category drop-down box.

The following information appears:

> Unknown IE (cGgsnIeUnknownRejPdps)

> Out of Order IE (cGgsnIeOutOfOrderRejPdps)

> IE Unexpected (cGgsnIeUnexpectedRejPdps)

> IE Duplicated (cGgsnIeDuplicatedRejPdps)

> Optional IE Incorrect (cGgsnOptIeIncorrectRejPdps)

> TFT already exists (cGgsnPdpWithoutTftExistsRejPdps)

##

### Unknown IE (cGgsnIeUnknownRejPdps)

The number of PDP contexts that rejected due to the cause of IE Unknown.

This counter is triggered by create/update PDP / PPP PDP context request message.

### Out of Order IE (cGgsnIeOutOfOrderRejPdps)

The number of PDP contexts that rejected due to the cause of IE Out of Order.

This counter is triggered by create/update PDP / PPP PDP context request message.

### IE Unexpected (cGgsnIeUnexpectedRejPdps)

The number of PDP contexts that rejected due to the cause of IE Unexpected.

This counter is triggered by create/update PDP / PPP PDP context request message.

### IE Duplicated (cGgsnIeDuplicatedRejPdps)

The number of PDP contexts that rejected due to the cause of IE Duplicated.

This counter is triggered by create/update PDP / PPP PDP context request message.

### Optional IE Incorrect (cGgsnOptIeIncorrectRejPdps)

The number of PDP contexts that rejected due to the cause of Optional IE Incorrect.

This counter is triggered by create/update PDP / PPP PDP context request message.

### TFT already exists (cGgsnPdpWithoutTftExistsRejPdps)

The number of PDP contexts that were rejected due to the cause of PDP context without TFT already exists.

This counter is triggered by create/update PDP / PPP PDP context request message.