# Home Agent Redundancy Statistics - Binding Information

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.

2. Select Home Agent Redundancy Statistics –Binding Information from the Category list.

The following information appears:

> Binding Info Received (cmiHaRedunReceivedBIReps)

> Replies Dropped (cmiHaRedunDroppedBIReps)

> Ack Sent (cmiHaRedunSentBIAcks)

> Requests Received (cmiHaRedunReceivedBIReqs)

> Requests Replies (cmiHaRedunSentBIReps)

> No Acknowledgement (cmiHaRedunFailedBIReps)

> Total Binding Info (cmiHaRedunTotalSentBIReps)

### Binding Info Received (cmiHaRedunReceivedBIReps)

The total number of binding information requests received by the home agent.

### Replies Dropped (cmiHaRedunDroppedBIReps)

The total number of binding information replies dropped since there is no corresponding binding information request sent by the home agent.

### Ack Sent (cmiHaRedunSentBIAcks)

The total number of acknowledgements sent in response to binding information replies received by the home agent.

### Requests Received (cmiHaRedunReceivedBIReqs)

The total number of binding information requests received by the home agent.

### Requests Replies (cmiHaRedunSentBIReps)

The total number of binding information replies sent by the home agent.

### No Acknowledgement (cmiHaRedunFailedBIReps)

The total number of binding information replies sent by by the home agent for which no acknowledgement is received from the standby home agent.

### Total Binding Info (cmiHaRedunTotalSentBIReps)

The total number of binding information replies sent by the home agent including retransmissions of the same reply.