# CDMA PDSN PPP Setup Statistics

This dialog box is applicable to Member and Peer to Peer clusters. From here, you can view valid and accepted point-to-point protocol (PPP) setup requests.

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN PPP Setup Statistics.

The following data is displayed:

> Currently Active PPP Connections (cCdmaPppCurrentConnections)

> PPP Initiate Connection Reqs Sent (cCdmaPppConnectionInitiateReqs)

> PPP Connection Reqs Succeessfully Active (cCdmaPppConnectionSuccesses)

> PPP Connections Entering LCP stage (cCdmaPppEnterLcpNums)

> PPP Connections Entering AUTH stage (cCdmaPppEnterAuthNums)

> PPP Connections Entering IPCP stage (cCdmaPppEnterIpcpNums)

### Currently Active PPP Connections (cCdmaPppCurrentConnections)

Number of active PPP connections.

### PPP Initiate Connection Reqs Sent (cCdmaPppConnectionInitiateReqs)

Number of PPP connection initiation requests sent out since system startup.

### PPP Connection Reqs Successfully Active (cCdmaPppConnectionSuccesses)

Number of PPP connections made active since system startup.

### PPP Connections Entering LCP stage (cCdmaPppEnterLcpNums)

Number of PPP connections entering the LCP stage since system startup.

### PPP Connections Entering AUTH stage (cCdmaPppEnterAuthNums)

Number of PPP connections entering the authentication stage since system startup.

### PPP Connections Entering IPCP stage (cCdmaPppEnterIpcpNums)

Number of PPP connections entering the IPCP stage since system startup.