# CDMA PDSN Update Failures

Use this option to view registration updates that are rejected.

## Procedure

To access CDMA PDSN registration failure information:

1. Right-click the device and select Monitor from the popup menu.

> > Monitor device dialog box appears.

2. Select CDMA PDSN Registration Update Failures from the Category menu.

CDMA PDSN Update Failures dialog box displays:

Update Request Failed Unspecified (cCdmaRpUpdReasonUnSpecFailures)

Update Request Failed Administrative (cCdmaRpUpdAdminProhibFailures)

Update Request Failed MN Authentication (cCdmaRpUpdMNAuthenFailures)

Update Request Failed Identity Mismatch (cCdmaRpUpdIdentMismatchFailures)

Update Request Failed Poor Request (cCdmaRpUpdBadReqFailures)

### Update Request Failed Unspecified (cCdmaRpUpdReasonUnSpecFailures)

Number of updated registration requests that failed since system startup for an unspecified reason.

### Update Request Failed Administrative (cCdmaRpUpdAdminProhibFailures)

Number of updated registration requests that failed since system startup due to administrative prohibition.

### Update Request Failed MN Authentication (cCdmaRpUpdMNAuthenFailures)

Number of updated registration requests that failed since system startup due to MN authentication failure.

### Update Request Failed Identity Mismatch (cCdmaRpUpdIdentMismatchFailures)

Number of updated registration requests that failed since system startup due to registration identity mismatch.

### Update Request Failed Poor Request (cCdmaRpUpdBadReqFailures)

Number of registration requests that failed since system startup due to poorly formed requests.