# Configuration Status

The values of the Configuration Status objects reflect the status of the configuration database.

Running Last Changed

Running Last Saved

Startup Last Changed

Maximum Event Entries

Entries Bumped

This category is available only on devices that support Cisco IOS Release 11.1 or later.

# Running Last Changed

The value of sysUpTime when the running configuration was last changed.

If the value of ccmHistoryRunningLastChanged is greater than ccmHistoryRunningLastSaved, the configuration has been changed but not saved.

# Running Last Saved

The value of sysUpTime when the running configuration was last saved (written).

If the value of ccmHistoryRunningLastChanged is greater than ccmHistoryRunningLastSaved, the configuration has been changed but not saved.

# Startup Last Changed

The value of sysUpTime when the startup configuration was last written to. In general, this is the default configuration used when cold starting the system. It could have been changed by a save of the running configuration or by a copy from elsewhere.

# Maximum Event Entries

The maximum number of entries that can be held in ccmHistoryEventTable. The recommended value for implementations is 10.

# Event Entries Bumped

The number of times the oldest entry in ccmHistoryEventTable was deleted to make room for a new entry.