# Home Agent Registration Processing Configs

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. Select category Home Agent Registration Processing Configs.

The following information appears:

> Max Registration Processed (cmiHaRegDateMaxRegsProcLoc)

> Max Registration Processed by AAA (cmiHaRegDateMaxRegsProcByAAA)

> Average Processing Time (cmiHaRegAvgTimeRegsProcByAAA)

> Maximum Processing Time (cmiHaRegMaxTimeRegsProcByAAA)

### Max Registration Processed (cmiHaRegDateMaxRegsProcLoc)

The time at which the number of registration requests processed in a minute by the home agent reached maximum. Includes only those registration requests that were authenticated locally by the home agent.

### Max Registration Processed by AAA (cmiHaRegDateMaxRegsProcByAAA)

The time at which number of registration requests processed in a minute by the home agent reached maximum. Includes only those registration requests that were authenticated by the AAA server.

### Average Processing Time (cmiHaRegAvgTimeRegsProcByAAA)

The average time taken by the home agent to process a registration request. Calculated based on those registration requests that were authenticated by the AAA server only .

### Maximum Processing Time (cmiHaRegMaxTimeRegsProcByAAA)

The maximum time taken by the home agent to process a registration request. It considers only those registration requests that were authenticated by the AAA server.