# CPU Utilization Table

## Navigation

1. Right-click the Service and Application Module for IP (SAMI) card and then select Configure.
2. Select SAMI module from the Category drop-down box.
3. With a device selected, click Statistics.
4. Select CPU Utilization Table from the Category drop-down box.

The following information appears:

> CPU Index (cpmCPUTotalIndex)

> Entity Physical Index (cpmCPUTotalPhysicalIndex)

### CPU Index (cpmCPUTotalIndex)

Index that uniquely represents a CPU (or group of CPUs) whose CPU load information is reported by a row in this table. This index is assigned arbitrarily by the engine and is not saved after a reboot.

### Entity Physical Index (cpmCPUTotalPhysicalIndex)

entPhysicalIndex value of the physical entity for which the CPU statistics in this entry are maintained. The physical entity can be a CPU chip, a group of CPUs, a CPU card, etc. The exact entity type is described by its entPhysicalVendorType value. If the CPU statistics in this entry correspond to more than one physical entity (or no physical entities), or if the entPhysicalTable is not supported by the SNMP agent, the value of this object must be zero.