# Displaying Card Configuration Information

To display card configuration information, double-click the card. The CiscoView configure card window appears. The display may vary, depending upon the card type. The fields listed below are typical.

> Index (cardIndex)

> Type (cardType)

> Description (cardDescr)

> Serial Number (cardSerial)

> Hardware Version (c ardHwVersion)

> Software Version (cardSwVersion)

> Slot Number (cardSlotNumber)

For some cards, you can get additional information by selecting the card type from the CATEGORY pulldown menu. Two examples of card types with additional fields are FDDI station management for FDDI cards, and CSA card configuration information for the CSA card.

Index (cardIndex)

Displays the index information of the card table.

Type (cardType)

The functional type of the card.

Description (cardDescr)

A text description of the card.

Serial Number (cardSerial)

The serial number of the card.

Hardware Version (cardHwVersion)

The hardware revision level of the card.

Software Version (cardSwVersion)

Version of firmware or microcode installed on the card.

Slot Number (cardSlotNumber)

Slot number relative to the containing card or chassis. It is -1 if neither applicable nor determinable.