# Home Agent Registration Processing Statistics -Initial Registration

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Statistics button.

4. Select category Home Agent registration Processing Statistics-Initial Registration.

The following information appears:

> No Encap (cmiHaEncapUnavailable)

> NAI Check Fails (cmiHaNAICheckFailures)

> Init Request Received (cmiHaInitRegRequestsReceived)

> Init Request Accepted (cmiHaInitRegRequestsAccepted)

> Init Request Denied (cmiHaInitRegRequestsDenied)

> Init Request Discarded (cmiHaInitRegRequestsDiscarded)

> MB Table Entries (cmiHaRegTotalMobilityBindings)

### No Encap (cmiHaEncapUnavailable)

Total number of registration requests denied by the home agent due to an unsupported encapsulation.

### NAI Check Fails (cmiHaNAICheckFailures)

Total number of registration requests denied by the home agent due to an NAI check failures.

### Init Request Received (cmiHaInitRegRequestsReceived)

Total number of initial registration requests received by the home agent.

### Init Requests Accepted (cmiHaInitRegRequestsAccepted)

Total number of initial registration requests accepted by the home agent.

### Init Request Denied (cmiHaInitRegRequestsDenied)

Total number of initial registration requests denied by the home agent. Reasons that a home agent denies a request include:

1. Can't allocate IP address for MN.
2. Request parsing failed.
3. NAI length exceeds the packet length.

### Init Request Discarded (cmiHaInitRegRequestsDiscarded)

Total number of initial registration requests discarded by the home agent. Reasons that a home agent discards a request include:

1. IP mobile home-agent service is not enabled.
2. HA-CHAP authentication failed.
3. Mobile node security association retrieval failed.

### MB Table Entries (cmiHaRegTotalMobilityBindings)

Current number of entries in haMobilityBindingTable. The haMobilityBindingTable contains the home agent's mobility binding list. The home agent updates this table in response to registration events from mobile nodes.