# Attach ACLs

Configuration > Interfaces > Attach ACLs

This dialog box lists the current mappings of ACLs to particular interfaces. From here, you can launch dialog boxes to create new mappings.

Note: To delete the mapping of an ACL to an interface, you must use the Command Line Interface (CLI).

For the description of a particular column heading in this dialog box, click the appropriate link from the following list:

- ACL Type

- ACL Name

- Port(s)

- VLAN(s)

The following list specifies buttons in this dialog box, as well as their function:

- Click New IP ACL Mapping to launch the Attaching IP ACL to Interfaces dialog box.

- Click New IPX ACL Mapping to launch the Attaching IPX ACL to Interfaces dialog box.

- Click New MAC ACL Mapping to launch the Attaching MAC ACL to Interfaces dialog box.

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access the online help.

ACL Type

Specifies the interface type for a Access Control List (ACL): IP, IPX, or MAC.

ACL Name

The name of an ACL.

Port(s)

The ports on which ACL is configured.

VLAN(s)

The VLAN an ACL belongs to.