# PPPoE

The PPPoE dialog provides details of the established PPPoE sessions within the system.

## Procedure

Right-click the device, then select PPPoE.

The following information appears:

> Active Sessions (cPppoeSystemCurrSessions)

> High Water Mark Established (cPppoeSystemHighWaterSessions)

> Maximum Allowed Sessions (cPppoeSystemMaxAllowedSessions)

> Threshold Value (cPppoeSystemThresholdSessions)

## Related Topics

PPPoE VCL Sessions

### Active Sessions (cPppoeSystemCurrSessions)

The current number of active PPPoE sessions within this system.

### High Water Mark Established (cPppoeSystemHighWaterSessions)

The high water mark of the established PPPoE sessions since the system was initialized.

### Maximum Allowed Sessions (cPppoeSystemMaxAllowedSessions)

Maximum number of allowed PPPoE sessions within the system.

### Threshold Value (cPppoeSystemThresholdSessions)

Threshold value of the established PPPoE sessions within the system. Default value is equal to cPppoeSystemMaxAllowedSessions.