Summer Time

# Summer Time

Device>Configure>Summer Time

This feature allows the user to specify the local dates and time, the summer time start and end as well as summer time recurring start and end. After selecting and invoking Summer Time menu in the device configuration menu, the following dialog window will be shown up and the user can perform summer time configuration.

Country Location (csyLocationCountry)

The country where the system is physically located (enter only 2 characters using A-Z. For example, for the United States of America enter US, for United Kingdom enter UK, for China enter CN, for Taiwan Province of China enter TW).

Summer Time Status (csySummertimeStatus)

An indication of whether the summer time is enabled on this device.

Summer Time Offset (csySummerTimeOffset)

The value of this object indicates number of minutes to add or to subtract during summer time.

csyClockDateAndTime

The current local date and time for the system. (YYYY-MM-DD, HH:MM. For example, 2000-01-14, 12:33)

csySummerTimeRecurringStart

This field indicates that summer time starts at this time every week. Indicate the week of the month, the day of the week, the month and the time. (W-DAY-MM, HH:MM. For example, 1-Sun-Jan, 12:33)

csySummerTimeRecurringEnd

This field indicates that summer time ends at this time every week. Indicate the week of the month, the day of the week, the month and the time. (W-DAY-MM, HH:MM. For example, 1-Sun-Jan, 12:33)