# COPS Servers Device Configuration

Device>Configure>Cops>Servers

Server Name (ccopsServerConfigName)

The IP address or the hostname of a COPS server.

Server Client Type (ccopsServerConfigClientType)

The type of policies to be retrieved from this server.

Server Table Entry Priority (ccopsServerConfigPriority)

The priority of this entry is relative to other entries when two entries of the same ccopsServerConfigClientType have the same ccopsServerConfigPriority value. The first one displayed in the table has the higher priority.

Destination Port (ccopsServerConfigPort)

The destination port number to which COPS server messages should be sent. By default the COPS service will be provided on the well-known COPS protocol port number 3288.

Click Create to add an entry to this table.

Select an entry and click Delete to delete an entry from this table.