# Monitoring DS3 Current Statistics

Select DS3 Current Statistics from the Monitor pull-down menu to monitor the following values:

P-bit Erred Secs (dsx3CurrentPESs)

P-bit Severely Erred Secs (dsx3CurrentPSESs)

Severely Erred Framing Secs (dsx3CurrentSEFSs)

Unavail Secs (dsx3CurrentUASs)

Line Coding Violates (dsx3CurrentLCVs)

P-bit Coding Violates (dsx3CurrentPCVs)

Line Erred Secs (dsx3CurrentLESs)

# P-bit Erred Secs (dsx3CurrentPESs)

The number of seconds in the current 15-minute interval during which P-bit errors occurred.

# P-bit Severely Erred Secs (dsx3CurrentPSESs)

The number of seconds in the current 15-minute interval during which severe P-bit errors occurred.

# Severely Erred Framing Secs (dsx3CurrentSEFSs)

The number of seconds in the current 15-minute interval during which severe framing errors occurred.

# Unavail Secs (dsx3CurrentUASs)

The number of seconds in the current 15-minute interval during which DS3 service was unavailable.

# Line Coding Violates (dsx3CurrentLCVs)

The number of line coding violations counted in the current 15-minute interval.

# P-bit Coding Violates (dsx3CurrentPCVs)

The number of P-bit coding violations counted in the current 15-minute interval.

# Line Erred Secs (dsx3CurrentLESs)

The number of seconds in the current 15-minute interval during which line errors occurred.