# Foreign Agent Registration Statistics1

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select Foreign Agent Registration Statistics1.

The following information is displayed:

> Regn Requests Count Total (faRegRequestsReceived)

> Regn Requests Relayed (faRegRequestsRelayed)

> Reason Unspecified Regns Rejected (faReasonUnspecified)

> Administratively Prohibited Regns (faAdmProhibited)

> Insufficient Resources - Regns Rejected (faInsufficientResource)

> Authentication Failure - Regns Rejected (faMNAuthenticationFailure)

> Long Lifetime - Regns Rejected (faRegLifetimeTooLong)

> Poorly formed Requests (faPoorlyFormedRequests)

### Regn Requests Count Total (faRegRequestsReceived)

Total number of valid registration requests received.

### Regn Requests Relayed (faRegRequestsRelayed)

Total number of registration requests relayed to the home agent by the foreign agent.

### Reason Unspecified Regns Rejected (faReasonUnspecified)

Total number of registration requests denied by the foreign agent—reason unspecified (code 64).

### Administratively Prohibited Regns (faAdmProhibited)

Total number of registration requests denied by the foreign agent—administratively prohibited (code 65).

### Insufficient Resources - Regns Rejected (faInsufficientResource)

Total number of registration requests denied by the foreign agent—insufficient resources (code 66).

### Authentication Failure - Regns Rejected (faMNAuthenticationFailure)

Total number of registration requests denied by the foreign agent—mobile node failed authentication (code 67).

### Long Lifetime - Regns Rejected (faRegLifetimeTooLong)

Total number of registration requests denied by the foreign agent—requested lifetime too long (code 69).

### Poorly formed Requests (faPoorlyFormedRequests)

Total number of registration requests denied by the foreign agent—poorly formed request (code 70).