# Monitoring DS3 Total Statistics

Select DS3 Total Statistics from the Monitor pull-down menu to monitor the following values:

P-bit Erred Secs (dsx3TotalPESs)

P-bit Severely Erred Secs (dsx3TotalPSESs)

Severely Erred Framing Secs (dsx3TotalSEFSs)

Unavail Secs (dsx3TotalUASs)

Line Coding Violates (dsx3TotalLCVs)

P-bit Coding Violates (dsx3TotalPCVs)

Line Erred Secs (dsx3TotalLESs)

# P-bit Erred Secs (dsx3TotalPESs)

The number of seconds in the current 15-minute interval during which P-bit errors occurred.

# P-bit Severely Erred Secs (dsx3TotalPSESs)

The number of seconds in the current 15-minute interval during which severe P-bit errors occurred.

# Severely Erred Framing Secs (dsx3TotalSEFSs)

The number of seconds in the current 15-minute interval during which severe framing errors occurred.

# Unavail Secs (dsx3TotalUASs)

The number of seconds in the current 15-minute interval during which DS3 service was unavailable.

# Line Coding Violates (dsx3TotalLCVs)

The number of line coding violations counted in the current 15-minute interval.

# P-bit Coding Violates (dsx3TotalPCVs)

The number of P-bit coding violations counted in the current 15-minute interval.

# Line Erred Secs (dsx3TotalLESs)

The number of seconds in the current 15-minute interval during which line errors occurred.