# Billing Mediation Agent Statistics2

## Navigation

1. Right-click the Service and Application Module for IP (SAMI) card and then select Configure.
2. Select SAMI module from the Category drop-down box.
3. With a device selected, click Statistics.
4. Select Content Services Gateway from the Category drop-down box.
5. Select Billing Agent from the Category drop-down box.
6. With a table entry selected, click Monitor.
7. Select Billing Mediation Agent Statistics2 from the Category drop-down box.

The following information appears:

> Messages to be ACKed (ccsBMAOutstanding)

> Time to Reset High Water (ccsBMAHighWaterResetTime)

> Bad Records Received (ccsBMABadRecord)

> Max Bad Records Received (ccsBMAHCBadRecord)

> Messages Retransmitted (ccsBMARetransmit)

> Max Messages to BMA (ccsBMAHCRetransmit)

### Messages to be ACKed (ccsBMAOutstanding)

Current number of messages waiting to be acknowledged.

### Time to Reset High Water (ccsBMAHighWaterResetTime)

Indicates when ccsBMAHighWater was last reset to zero.

### Bad Records Recieved (ccsBMABadRecord)

Number of bad records received. These are records in which an error was detected while attempting to decode its contents.

### Max Bad Records Received (ccsBMAHCBadRecord)

Number of bad records received. These are records in which an error was detected while attempting to decode its contents.

This object is a 64-bit version of ccsBMABadRecord.

### Messages Retransmitted (ccsBMARetransmit)

Number of messages retransmitted to the billing mediation agent (BMA).

### Max Messages to BMA (ccsBMAHCRetransmit)

Number of messages retransmitted to the BMA.

This object is a 64-bit version of ccsBMARetransmit.