# RP Update Statistics Info

Use this option to view valid and accepted request statistics.

## Procedure

To access RP update statistics information:

Right-click the device and select Monitor from the popup menu.

RP Update Statistics Info dialog box displays:

Update Request Received (cCdmaRPUpdValidRequests)

Update Request Accepted (cCdmaRPUpdAcceptedReplies)

Update Request Failed Unspecified (cCdmaRPUpdReasonUnSpecFailures)

Update Request Failed Administrative (cCdmaRPUpdAdminProhibFailures)

Update Request Failed MN Authentication (cCdmaRPUpdMNAuthenFailures)

Request Failed Identity Mismatch (cCdmaRPUpdIdentMismatchFailures)

Request Failed Poor Request (cCdmaRPUpdBadRequestFailures)

## Related Topics

CDMA PDSN Feature Overview

CDMA PDSN System Statistics

CDMA PDSN PCF Statistics

CDMA PDSN Session Statistics

Registration Statistics

### Update Request Received (cCdmaRPUpdValidRequests)

Number of valid, updated registration requests received since system startup.

### Update Request Accepted (cCdmaRPUpdAcceptedReplies)

Number of valid, updated, registration replies accepted since system startup.

### Update Request Failed Failed Unspecified (cCdmaRPUpdReasonUnSpecFailures)

Number of updated registrations failed for unspecified reason since system startup.

### Update Request Failed Administrative (cCdmaRPUpdAdminProhibFailures)

Number of updated registrations failed due to administrative prohibition since system startup.

### Update Request Failed MN Authentication (cCdmaRPUpdMNAuthenFailures)

Number of updated registrations failed due to MN authentication failure since system startup.

### Request Failed Identity Mismatch (cCdmaRPUpdIdentMismatchFailures)

Number of registrations failed due to registration identity mismatch since system startup.

### Request Failed Poor Request (cCdmaRPUpdBadRequestFailures)

Number of updated registrations failed due to poorly formed request since system startup.