# SAMI Module

## Navigation

1. Right-click the Service and Application Module for IP (SAMI) card and then select Configure.
2. Select SAMI module from the Category drop-down box.

The following information appears:

> Device ID (cdpCacheDeviceId)

> Address (cdpCacheAddress)

> Device Platform (cdpCachePlatform)

With a device selected, click Statistics to launch the CPU Utilization Table dialog box.

### Device ID (cdpCacheDeviceId)

Device identifier string, as reported in the most recent CDP message. A zero-length string indicates that no Device ID field (TLV) was reported.

### Address (cdpCacheAddress)

First network-layer address of the SNMP agent on the device, as reported in the most recent CDP message. For example, if the corresponding instance of cacheAddressType has a value of ip(1), then this object is an IP address.

### Device Platform (cdpCachePlatform)

Hardware platform of the device, as reported in the most recent CDP message. A zero-length string indicates that no Platform field (TLV) was reported.