# Mobility Agent Advertisement Table

The table displays the following information:

Source IpAddress (maInterfaceAddress)

Max Registration Lifetime (maAdvMaxRegLifetime)

PrefixLength Extension (maAdvPrefixLengthInclusion)

Destination IpAddress (maAdvAddress)

Max Advertisement Interval (maAdvMaxInterval)

Min Advertisement Interval(maAdvMinInterval)

Max Advertisement Lifetime (maAdvMaxAdvLifetime)

Advertise On Solicitation (maAdvResponseSolicitationOnly)

Row Status(maAdvStatus)

### Source IpAddress (maInterfaceAddress)

IP adddress for advertisement interface.

### Max Registration Lifetime (maAdvMaxRegLifetime)

The longest lifetime, in seconds, that the mobility agent is willing to accept in any Registration Request.

### PrefixLength Extension (maAdvPrefixLengthInclusion)

Indicates whether the advertisements send over the interface includes Prefix-Lengths extension.

Possible values are:

true | All advertisements includes the Prefix-Lengths extension.
false | All advertisemens need not include the Prefix-Lengths extensions.

### Destination IpAddress (maAdvAddress)

The IP destination address to be used for advertisements sent from the interface.

The only permissible values are the all-systems multicast address (224.0.0.1) or the limited-broadcast address

(255.255.255.255)

### Max Advertisement Interval (maAdvMaxInterval)

Maximum time interval, in seconds, between successive transmissions of Agent Advertisement from the interface.

### Min Advertisement Interval(maAdvMinInterval)

Minimum time interval, in seconds, between successive transmission of Agent Advertisements from the interface.

### Max Advertisement Lifetime (maAdvMaxAdvLifetime)

Time, in seconds, to be placed in the lifetime field of the RFC 1256-portion of the agent advertisement sent over the interface.

### Advertise On Solicitation (maAdvResponseSolicitationOnly)

Indicates whether the advertisement from the interface should be send only in response to an agent solicitation message.

### Row Status(maAdvStatus)

Row satus for the agent advertisement table. If the column status is 'active', the manager should not change any column in the row.