# NTP

Device>Configure>NTP

Use the NTP dialog box to set Network Time Protocol (NTP) parameters for the device.

Using NTP Server (ntpBcastClient)

Whether this device should act as a broadcast client.

Broadcast Delay (ntpBcastDelay)

Estimated round trip time (in microseconds) for NTP broadcasts.

Receiving NTP Broadcast (ntpClient)

Whether this device should act as an NTP client in a client-server configuration.

Regular Time Zone Name (ntpTimezoneName)

Your time zone name, for display purposes.

Time Offset Hour(s) (ntpTimezoneOffsetHour)

Number of hours that your time zone is offset from Greenwich Mean Time (GMT).

Time Offset Minute(s) (ntpTimezoneOffsetMinute)

Number of minutes that your time zone is offset from Greenwich Mean Time (GMT).

Summer Time (ntpSummertimeStatus)

Whether your clock should be set ahead one hour for summer time (such as Daylight Savings Time in the USA).

More Summer Time configuration options are available under Device Configuration.

Summer Time Zone Name (ntpSummerTimezoneName)

Your summer time zone name, for display purposes.

Click Apply to make your changes to these eight values take effect.

NTP Server's IP (ntpServerAddress)

IP address of this NTP server.

Click Create to add a new entry to this table, or click Delete to remove the selected entry.

Click Cancel to close the dialog box without making any changes. Click Print to print the contents of the dialog box.