# SLB Statistics (64-bit)

To access the SLB Statistics dialog box:

1. Select Device > Configure > SLB Statistics.

2. With a server load balancing (SLB) instance selected, click 64 Bit Monitor.

This dialog box displays the following data:

- Packet Forwarded-64bit (slbStatsUnassistedSwitchingHCPks)

- Packets Handled-64bit (slbStatsAssistedSwitchingHCPkts)

- Connections Created-64 bit (slbStatsCreatedHCConnections)

- Connections Established-64bit (slbStatsEstablishedHCConnections)

- Connections Destroyed-64bit (slbStatsDestroyedHCConnections)

- Connections Reassinged-64bit (slbStatsReassignedHCConnections)

- Connections Zombie-64bit (slbStatsHCZombies)

The following list specifies buttons in this dialog box, as well as their function:

- To specify the refresh rate for this dialog box, select a value from the drop-down box.

- Click Start/Stop to begin/end device monitoring.

> Note: The Start/Stop toggle feature is supported only by CiscoView 5.x.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Packet Forwarded-64bit (slbStatsUnassistedSwitchingHCPks)

The number of packets forwarded by the SLB manager software. This is the 64-bit version of slbStatsUnassistedSwitchingPkts.

Packets Handled-64bit (slbStatsAssistedSwitchingHCPkts)

The number of packets switched via the highest-performance switching path. This is the 64-bit version of slbStatsAssistedSwitchingPkts.

Connections Created-64 bit (slbStatsCreatedHCConnections)

The number of connections SLB created since it was configured. TCP connections are created after seeing a SYN for a connection. UDP connections are created based on the source and destination, and are removed based on a timer. This is the 64-bit version of slbStatsCreatedConnections.

Connections Established-64bit (slbStatsEstablishedHCConnections)

The number of connections established through SLB. TCP connections reach the ESTAB state after a SYN - SYN/ACK exchange. UDP connections reach the ESTAB state after data is sent from the client or server.

Connections Destroyed-64bit (slbStatsDestroyedHCConnections)

The number of TCP and UDP connections SLB destroyed, either by TCP/IP teardown or timeout. UDP connections can only be timed out. This is the 64-bit version of slbStatsDestroyedConnections.

Connections Reassinged-64bit (slbStatsReassignedHCConnections)

The number of TCP and UDP connections reassigned from one real server to another. This is the 64-bit version of slbStatsReassignedConnections.

Connections Zombie-64bit (slbStatsHCZombies)

The number of TCP and UDP connections currently in the zombie state waiting for timers to expire. This is the 64-bit version of slbStatsZombies.