# CDMA PDSN Update Additional Statistics

Use this option to view valid and accepted registration updates.

## Procedure

To access CDMA PDSN update statistics information:

1. Right-click the device and select Monitor from the popup menu.

> > Monitor device dialog box appears.

2. Select CDMA PDSN Update Additional Statistics from the Category menu.

CDMA PDSN Update Additional Statistics dialog box displays:

Registration Update Acks Received (cCdmaRpUpdReceivedAcks)

Registration Update Acks Discarded(cCdmaRpUpdDiscardedAcks)

Registration Update Reqs - Lifetime Expiry (cCdmaRpUpdRpLifeExpReqs)

Registration Update Reqs - PPP Termination(cCdmaRpUpdPPPtermReqs)

Registration Update Reqs – Other Reason(cCdmaRpUpdOtherReasonReqs)

### Registration Update Acks Received (cCdmaRpUpdReceivedAcks)

Number of A-11 registration acknowledgements received since system startup.

### Registration Update Acks Discarded (cCdmaRpUpdDiscardedAcks)

Number of A-11 registration acknowledgements discarded since system startup.

### Registration Update Reqs - Lifetime Expiry (cCdmaRpUpdRpLifeExpReqs)

Number of initial A-11 registration updates since system startup due to RP lifetime expiration.

Note: This count does not include any re-transmissions.

### Registration Update Reqs - PPP Termination (cCdmaRpUpdPPPtermReqs)

Number of initial A-11 registration updates sent as a result of PPP termination since system startup.

Note: This count does not include any re-transmissions.

The code field in the registration reply message is set to non-zero.

### Registration Update Reqs – Other Reason (cCdmaRpUpdOtherReasonReqs)

Number of initial A-11 registration updates sent due to reasons other than RP lifetime expiry or PPP termination since system startup.

Note: This count does not include any re-transmissions.