# CSG Quota Manager Statistics1

## Navigation

1. Right-click the Service and Application Module for IP (SAMI) card and then select Configure.
2. Select SAMI module from the Category drop-down box.
3. With a device selected, click Statistics.
4. Select Content Services Gateway from the Category drop-down box.
5. Select CSG Quota Server from the Category drop-down box.
6. With a table entry selected, click Monitor.
7. Select CSG Quota Manager Statistics1 from the Category drop-down box.

The following information appears:

> Records Lost (ccsQuotaMgrLostRecords)

> Max Records Lost (ccsQuotaMgrHCLostRecords)

> Records Sent (ccsQuotaMgrTotalSent)

> Total Records Sent (ccsQuotaMgrHCTotalSent)

> Ackmts Received (ccsQuotaMgrFailAck)

> Max Ackmts Received (ccsQuotaMgrHCFailAck)

### Records Lost (ccsQuotaMgrLostRecords)

Total number of lost records since system initialization or the last time the counter wrapped.

### Max Records Lost (ccsQuotaMgrHCLostRecords)

Total number of lost records since system initialization or the last time the counter wrapped.

This object is a 64-bit version of ccsQuotaMgrLostRecords.

### Records Sent (ccsQuotaMgrTotalSent)

Total number of records sent to the quota manager.

### Total Records Sent (ccsQuotaMgrHCTotalSent)

Total number of records sent to the quota manager.

This object is a 64-bit version of ccsQuotaMgrTotalSent.

### Ackmts Received (ccsQuotaMgrFailAck)

Number of acknowledgments received from the quota manager for which there are no requests.

### Max Ackmts Received (ccsQuotaMgrHCFailAck)

Number of acknowledgments received from the quota manager for which there are no requests.

This object is a 64-bit version of ccsQuotaMgrFailAck.