# Foreign Agent Asymmetric Link Support

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.

2. Select Foreign Agent Asymmetric Link Support Configs from the Category list.

3. Select a row and click the Monitor button.

The following information appears:

> Registration Requests Received for CoA (cmiFaCoaRegAsymLink)

### Registration Requests Received for CoA (cmiFaCoaRegAsymLink)

Specifies whether the foreign agent interface associated with this care-of-address (CoA) should advertise only this CoA or not. If it is true, other configured care-of-addresses will not be advertised.