# Status Information for GGSN

Use this option to view status information for GGSN.

## Procedure

1. Right-click the device and then select Monitor.

2. Select Status Information for GGSN from the Category list.

The following information appears:

Rx Packet Queue Size (cgprsGtpCurRxPacketQueueSize)

G-PDUs (cgprsGtpCurUnexpRxGpduCnt)

Rejected PDP Context (cgprsGtpCurRejPDPCxtActivationCnt)

Dropped Packets (cgprsGtpTotalPktsDropped)

Premium QoS Mean Throughput (cgprsGtpCurMTForPremiumQos)

Normal QoS Mean Throughput (cgprsGtpCurMTForNormalQos)

Best Effort QoS Mean Throughput (cgprsGtpCurMTForBestEffortQos)

x -Packets Y-Time (x-cgprsGtpDroppedPktsTimeFrame,y-cgprsGtpDroppedPktsCnt)

Rx Packet Queue Size (cgprsGtpCurRxPacketQueueSize)

Indicates the current size of the Rx packet queue on the GSN node.

G-PDUs (cgprsGtpCurUnexpRxGpduCnt)

Indicates the total number of G-PDUs received from a SGSN for a non-existing or inactive PDP context since system startup.

Rejected PDP Context (cgprsGtpCurRejPDPCxtActivationCnt)

Indicates the total number of rejected PDP context activations since system startup.

Dropped Packets (cgprsGtpTotalPktsDropped)

Indicates the number of packets dropped because of an unknown GTP header, since system startup.

Premium QoS Mean Throughput (cgprsGtpCurMTForPremiumQos)

Indicates the mean throughput, in bits per second, for premium class QoS users on the GSN.

Normal Qos Mean Throughput (cgprsGtpCurMTForNormalQos)

Indicates the mean throughput for normal class QoS users on the GSN.

Best Effort Qos Mean Throughput (cgprsGtpCurMTForBestEffortQos)

Indicates the mean throughput for 'best-effort' class QoS users on the GSN.

x-Packets Y-Time (x-cgprsGtpDroppedPktsTimeFrame,y-cgprsGtpDroppedPktsCnt)

Indicates how many packets are dropped within a particular timeframe. It is represented with a graph.

cgprsGtpDroppedPktsTimeFrame

Indicates the time frame within which the GTP packets defined by cgprsGtpDroppedPktscnt are dropped.

cgprsGtpDroppedPktsCnt

Indicates the number of packets dropped by GTPwithin cgprsGtpDroppedPktsTimeFrame.